Figure 2.4: Amplitude calibrated data at 22.3 GHz prior to self–calibration. Amplitudes (top) and phases (bottom) plotted against the uv–distance.

Figure 2.5: Observed (top) and “CLEAN” model (bottom) amplitudes after self– calibration.

Figure 2.6: Observed (top) and “CLEAN” model (bottom) phases after the self– calibration.

Figure 2.7: Observed (rows 1 and 3 from the top) and “CLEAN” model (rows 2 and 4 from the top) amplitudes projected onto different position angles. The position angles displayed are 0^∘, 30^∘, 60^∘, 86^∘, 120^∘, and 150^∘.